|  | Important notice

1. When you install the driver into the 1st Computer , please firstly install the software from the CD driver , and then put one end of the USB 2.0 Network cable into a USB Port in the 1st Computer , and leave the other end of the USB 2.0 Network cable unused .( Never connect it to any other computers ). ( Refer to image 1 )
(image 1)
2. When you put the USB 2.0 Network cable into a USB Port in the 1st Computer , system will detect it and start to install , just follow up the installation guide to install it .

3. After you install the 1st Computer , please pull out the USB 2.0 Network cable from the 1st Computer .

4. When you install the driver into the 2nd Computer , please firstly install the software from the CD driver , and then put one end of the USB 2.0 Network cable into a USB Port in the 2nd Computer , and leave the other end of the USB 2.0 Network cable unused ( Never connect it to any other computers ).
( Refer to image 2 )
( image 2)
5. When you put the USB 2.0 Network cable into a USB Port in the 2nd Computer , system will detect it and start to install , just follow up the installation guide to install it .

6. After you install the 2nd Computer , please pull out the USB 2.0 Network cable from the 2nd Computer .

7. Restart the both computers , and link the both Computers with USB 2.0 Network Cable , then you can run it . ( Refer to image 3 )

(image 3)

How to set up a local area network between 2 sets of computers?

1. After installing the driver for ‘ Networking', please re-start the 2 sets of computers. And then, connect them by a USB Network Cable.

2．Please kindly appoint an uniform work group for them, but different users' name.

3．.If want to execute the local area network, the computers should be installed with NetBEUI Protocol. When installing operation system Windows XP, it hasn't attached this protocol. So, the user should install it by hand. It lies in installing disk L:\VALUEADD\MSFT\NET\NETBEUI.

Note: NetBEUI (NBF) doesn't belong to a router protocol. So, it could only be suitable for network on a small scale. What's more, Microsoft Windows could not support this protocol any more. If the product supporter reminds you to install the protocol as a temporary solution, please kindly follow the methods below, to install NetBEUI in Windows XP

* Please copy nbf.sys to the road: %SYSTEMROOT%\SYSTEM32\DRIVERS\ .

* Please copy netnbf.inf to the road: %SYSTEMROOT%\INF\ .

* Please open “Local Area Connection Properties”, click “install”. Then it would begin installing NetBeUI Protocol.

4. When set up a local area network for 2 computers, Please kindly pay attention to the operation system.

Different operation systems, the users’ name and password would be set in different way.

(1) Windows 98SE ←→ Windows 98SE 2. Windows 98SE ←→ Windows ME 3. Windows ME ←→ Windows ME

The password would be chosen freely. When log in for the first time, please kindly click ‘ ok' only, not need to type password. Also, please don't click ‘ ESC' to log on, or USB Network cable could not run smoothly.

(2) Windows 98SE (or Windows ME) ←→ Windows 2000 5. Windows 98SE (or Windows ME) ←→ Windows XP

If your operation system is Windows 98SE ( or Windows ME), and want to visit another computer with Windows 2000 (or Windows XP), you should build for the former a visiting user name and password in the latter, to make sure the smoothly running of USB Network cable.

Note: How to build a visiting user name and password in Windows 2000 (or Windows XP)?

" Control Panel " → “Users and Passwords”→ “Add New User”

(3) Windows 2000 (or Windows XP) ←→ Windows 2000 (or Windows XP)

You should build for the former a visiting user name and password in the latter, to make sure the smoothly running of USB Network cable.

Installing Software
User's manual